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Figure 1: Shallow foundation (spread footing). Photo from TR Construction Omaha
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Figure 2: Raft foundation. Photo by Fons Heijnsbroek on Unsplash
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Figure 3: Soil properties based on SPT-N values. Table from Foundation engineering, 2d ed., by Ralph B. Peck
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Table 5.3 Penetration Resistance and Soil Properties on Basis
of the Standard Penetration Test

Sands Clays
(Fairly Reliable) (Rather Unreliable)
Number of Blows Relative Number of Blows
per ft, N Density per ft, N Consistency
Below 2 Very soft
04 Very loose 2-4 Soft
410 Loose 48 Medium
10-30 Medium 8-15 Stiff
30-50 Dense 15-30 Very stiff

Over 50 Very dense Qver 30 Hard





