	MAP DESIGN


	In this chapter you will learn all steps necessary to compose common maps from available map layers. One type of map that you will create is a choropleth map that color-codes polygons to convey information about areas. The second is a “point feature map” that uses point markers to display spatial patterns in point data. 

	

	Learning Objectives

	· Create choropleth maps
· Create group layers
· Create custom classes in a legend
	· Create point maps
· Create a point feature map based on a definition query

	

	Tutorial  3 .1

	

	CREATE CHOROPLETH MAPS


	3.1.1
	Open and save a map document

	3.1.2
	Add a layer

	3.1.3
	Change a layer’s name

	3.1.4
	Select a census attribute to display state population

	3.1.5
	Manually change class colors

	3.1.6
	Create a map layout

	

	Tutorial 3.1


	Create Choropleth Maps


	A choropleth map (as shown in the following figure) is a map in which polygon areas are colored or shaded to represent attribute values. In this tutorial you will use population data of Bangladesh to create choropleth maps.


	



	3.1.1 Open and save a map document


	1. On your desktop, click Start, All Programs, ArcGIS, ArcMap 10.2.2
2. In the ArcMap – Click File, click New, click Blank Map ,click OK.
3. Save the file as Ex 3.mxd in Practice folder\Final
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	Arc Map opens a map with no layer added. You will add the layer needed for the exercises next.


	3.1.2 Add a layer

	1. Click the Add Data button[image: ].
2. Navigate to  D:\CE-210\Tutorial 3-3\DATA \BGD_adm3.shp

	


   


	





	3.1.3 Change a layer’s name

	
1. Right-click the BGD_adm3 layer in the TOC.
2. Click Properties.
3. Click the General tab.
4. Type District of Bangladesh as the new layer name and click OK.

	


    


	
[image: ]


	3.1.4 Select a census attribute to display state population

	
1. Right-click the District Of Bangladesh layer in the TOC.
2. Click Properties.
3. Click the Symbology tab.
4. In the Show box, click Quantities and Graduated colors.
5. In the Fields box, click the Value drop-down list and Population. Do not change other default settings.
6. Click the Color Ramp drop-down list, scroll down, and click the yellow-to-green-to-red color ramp.
7. Click OK.


	

 


	3.1.5 Manually change class colors

	
1. Turn on and Right-click the population layer and click Properties.
2. In the Layer Properties dialogue box, click the Symbology tab.
3. Click the Color Ramp drop-down list and scroll to and click the last color ramp.
4. Right-click the color Ramp and select Properties. 
5. Click the color box beside Color 1 and click the Arctic White paint chip.
6. Click the color box beside Color 2, click the Dark Navy paint chip, and click OK twice.
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3.1.6 Create a map layout 

	Create a map layout with appropriate notations. (You can keep default color ramp or can change color manually)

	[image: ][image: ]

	

	Tutorial  3.2


	Create Group Layers

	3.2.1
	Add a group layer to the map 

	3.2.2
	Add a layer to the group

	3.2.3
	Saving layer file


		

	Tutorial 3.2


	Create Group Layers

	Group layers contain other layers allowing for better organization of the layers in your map. Group layers have behavior similar to other layers in the TOC. Turning off the visibility of a group layer turns off the visibility of all its component layers.


	3.2.1 Add a group layer to the map

1. Right-click layers in the TOC.
2. Click New Group Layer.
3. Right-click the resulting New Group Layer and click Properties.
4. Click the General tab.
5. Type as the group layer name “Thana Of Bangladesh”( but do not click OK)

	


             

	
3.2.2 Add a layer to the group

1. Click the Group tab in the Group Layer Properties window.
2. Click the Add button and navigate to  D:\CE-210\Tutorial 3-3\DATA of Bangladesh
3. Click BD_HQ_Thana and click Add and OK.

	


    

	
3.2.3 Saving layer file

1. Right-click the District Of Bangladesh layer group and click Save As Layer File.
2. Navigate to the Home-CE-210\Practice.
3. Type District of Bangladesh .lyr in the Name field.
4. Click Save.

	

  

	





	
Tutorial  3.3


	Create choropleth map using custom attribute scales

	3.3.1 
	Classification method: Natural Breaks

	3.3.2 
	Classification method: Manual

	3.3.3 
	Classification method: Quantile

	3.3.4 
	Classification method: Geometric Interval

	3.3.5 
	Classification method: Standard Deviation

	

	Tutorial 3.3


	Create choropleth map using custom attribute scales 


	3.3.1 Classification method: Natural Breaks

	1. Zoom to the full extent[image: ].
2. Right-click the District Of Bangladesh and click Properties.
3. In the Layer Properties dialogue box, click the Symbology tab.
4. In the classification panel, click the Classes drop-down list, select 6 and classify.
5. Keep the classification method as  Natural Breaks (Jenks)
6. Change the layer name as “Natural Breaks”.


	

      


	

	3.3.2 Classification method: Manual
1. Click the Add Data button[image: ].
2. Navigate to  D:\CE-210\Tutorial 3-3\DATA \BGD_adm3.shp
3. Change the layer name to “Manual”
4. Click the classify option and then from the drop-down list for the classification Method select Manual.
5. In the Break Values panel, click the fifth value.
6. Type 32,00,000 and press Enter.
7. Continue clicking the break values above the last one changed and enter the following:16,00,000; 8,00,000; 4,00,000.Let the first (minimum) value remain 2,98,120 and last (maximum) value remain 85,11,228.


	

       


	
     [image: ]


	8. Click the gray Label heading, and then click Format Labels.
9. In the Number Format dialogue box, select Show thousands separates and click OK.


	

  


	10. In the Label field of the Symbology tab, change the first value to 2,98,120 or less and the last label to 85,11,228 or more.
11. Click OK.
[image: ]


	3.3.3 Classification method: Quantile

1. Click the Add Data button[image: ].
2. Navigate to  D:\CE-210\Tutorial 3-3\DATA \BGD_adm3.shp
3. Change the layer name to “Quantile”
4. Zoom to the full extent[image: ].
5. Right-click the Quantile and click Properties.
6. In the Layer Properties dialogue box, click the Symbology tab.
7. In the classification panel, click the Classes drop-down list, select 2 and classify.
8. Select the classification method as Quantile.

	

   


	


	3.3.4 Classification method: Geometric Interval

1. Click the Add Data button[image: ].
2. Navigate to  D:\CE-210\Tutorial 3-3\DATA \BGD_adm3.shp
3. Change the layer name to “Geometric Interval”
4. Zoom to the full extent[image: ].
5. Right-click the Geometric Interval and click Properties.
6. In the Layer Properties dialogue box, click the Symbology tab.
7. In the classification panel, click the Classes drop-down list, select 10 and classify.
8. Select the classification method as Geometric Interval.


	



	



	3.3.5 Classification method: Standard Deviation

1. Click the Add Data button[image: ].
2. Navigate to  D:\CE-210\Tutorial 3-3\DATA \BGD_adm3.shp
3. Change the layer name to “Standard Deviation”
4. Zoom to the full extent[image: ].
5. Right-click the Standard Deviation and click Properties.
6. In the Layer Properties dialogue box, click the Symbology tab.
7. In the classification panel, click  classify.
8. Select the classification method as  Standard Deviation
9. Break Classes at” as ½ Std. Dev.


	



	





	Tutorial  3.4


	Create point maps


	3.4.1
	Manually change the symbol

	3.4.2
	Create a point map based on definition query

	3.4.3
	Change a layer’s name and symbol

	


	Tutorial 3.4


	Create point maps


	Point maps show exact location of data or events using individual point markers for each event. You will create a point map (as shown in the following figure) showing Total Population of Bangladesh as points with size graduated point markers that represent total Population.

	


	3.4.1 Manually change the symbol

1. Add BGD_adm3.shp file.
2. Double-click in the   BGD_adm3.layer to open its Layer Properties window. 
3. Click the Symbology tab and change Quantities to Graduated Symbols.
4. In the Fields panel, change the Value to Population, symbol size to 2-10, the template symbol to a Dark Umber CIRCLE 1 and assign the break points and legend labels.
5. Click OK & zoom to the full extent.


	



	



	



	  


 


	3.4.2.1 Create a definition query


	3.4.2.1 Create a definition query

	1. Right-click the BD_HQ_Thana layer and click Properties. 
2. Click the Definition Query tab and Query Builder button. 
3. In the Query Builder window, double-click "THANACODE"
4. Click = as the logical operator. 
5. Click Get Unique Values. 
6. In the Unique Values list, double-click '94' and Click OK.


	

    


	



	

  


	

       



	3.4.3 Change a layer’s name and symbol

1. Right-click the BD_HQ_Thanalayer and click Properties. 
2. Click the General tab and change the name of the layer to THANACODE94
3. Click the Symbology tab to Features and the Symbol button.
4. Click the Circle 2 icon, change the color to Ultra Blue, and change the size to 10 & Click OK twice.
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